This distribution can be either installed from 1.44MB floppies or
from the hard disk drive.

FLOPPY INSTALL:
- Unzip the archive by executing the distribution file.  If you're
  reading this, you've already  done it.
- Format four 1.44MB (or greater) floppy drives.
- Copy the contents of each of the subdirectories (disk1, disk2,
  disk3, and disk4) onto the floppy drives.
- Insert disk1 into the drive.
- Go to the floppy drive by typeing A: (or B: if that's where your
  floppy drive is).
- Type INSTALL
- Read the readme file displayed.
- Select Install Product form the Action menu
- Choose the destination directory and Continue
- It is highly recommended that you allow the install program to
  update your config.sys for you.  A backup will be made automatically.
- As you are prompted for diskettes, place the appropriate diskette
  into the floppy drive.
- Remove the floppy from the floppy drive.
- Shutdown and reboot your computer

HARD DISK INSTALL
- Unzip the archive by executing the distribution file.  If you're
  reading this, you've already  done it.
- Change into the disk1 directory
- Type INSTALL
- Read the readme file displayed.
- Select Install Product form the Action menu
- Choose the destination directory and Continue
- It is highly recommended that you allow the install program to
  update your config.sys for you.  A backup will be made automatically.
- As you are prompted for diskettes, enter the correct directory name.
- Shutdown and reboot your computer

Mail:  SSESCO, 3490 Lexington Avenue North, Suite 110, Shoreview, MN 55126
Phone: (612) 481-0804
Fax:   (612) 481-0053
Email: info@SSESCO.com
FTP:   ftp://ftp.SSESCO.com
Web:   http://www.SSESCO.com
