### Embed using delay coordinates

`delay [-d# -m# -o` outfile`-l# -x# -c# -V# -h]` file

> `-d` delay (1)
> `-m` embedding dimension (2)
> `-l` number of values to be read (all)
> `-x` number of values to be skipped (0)
> `-c` column to be read (1 or file,#)
> `-o` output file name, just `-o` means file`_delay`
> `-V` verbosity level (0 = only fatal errors)
> `-h` show this message

Reads one column from a file and writes `m` delay coordinates as columns. Output file file`_delay`.

Table of Contents * TISEAN home