We offer CMS-C370VMa - a virtual machine designed for executing operational
system CMS that is a host operational system among the set of Virtual
Machines Monitor.

In the current version CP commands are not available except for:

#CP EXIT                - save status and exit CMS
#CP QUIT                - exit CMS without saving
#CP IPL <addr>          - load OS from device <addr>
#CP EXT <addr>          - interruption from device <addr>

In this version the full-screen mode is limited. This causes partial
availability of the HELP command (PF1) in XEDIT and FLIST, and in other
versions of CMS dialogs.

This limit disables usage of PF-keys in HELP mode, you should use command
lines.

In this version of C370VM statically defined table for 5 I/O devices is
available.

This version is designed for operational system OS/2. C370VM for other
operational systems is available only in commercial release.

This version is provided with customizing modes turned on to form large
log-files, that reduces the capacity of the system.

In this version of C370VM function of SMSG, IUCV, VMCF protocols support is
disabled.

In this version of C370VM function of SPOOL support is disabled. (Devices
RDR, PRT)

Contact the provider to enable these microcode functions.

In this version of C370VM function of NLSAMEN and shared blocks procedures
support is not available.

Loading:
Copy the folder DEMO from the CD with ESli emulator into the root directory
of any hard disk.

Run ESI.CMD in the command line of OS/2 from the folder \DEMO\CMS or folder
\DEMO\PDO\ on your hard disk.

Press ESC.

Enter command
        #cp i 190

You have loaded OS CMS or PDO, depending on the chosen folder.

Contacts with the developers: 7-(812)-532-5743,
chief engineer of "@E.P.A. Ltd."

e-mail: mail@epa.ru
