
IBM XGA-2 Butterfly Demo with New Graphic Images
------------------------------------------------

This package contains 10 zip files:

              XGAIBM1.zipbin
              XGAIBM2.zipbin
              XGAIBM3.zipbin
              XGAIBM4.zipbin
              XGAIBM5.zipbin
              XGAIBM6.zipbin
              XGAIBM7.zipbin
              XGAIBM8.zipbin
              XGAIBM9.zipbin
              XGAIBM10.zipbin

Procedure to set up demo:

  1. Download each file in binary to your PC
  2. Use PKUNZIP to decompress each file to diskette

     Note: PKUNZIP is available from the PCTOOLS disk in package PKZIBM.

  3. At the a:> type in install and follow directions

Prerequisites needed prior to installing demo:

  Running under a DOS operating system
  ------------------------------------

  Steps:

  1. XGA or XGA-2 must be installed on your PS/2 system

  2. the XGA DOS Adapter Interface (AI) driver must be installed;
     this driver is available from the DISPLAY tools disk or
     comes with the driver diskettes available with the XGA or
     XGA-2 card

  3. A 3MB RAMDRIVE (logical disk) must be set up;
     add the following line to config.sys....
     device=c:\dos\ramdrive.sys 3072 /e


  Running under OS/2 2.0 operating system
  -----------------------------------------

  Steps:

  -  Follow step 1 and 2 as described under DOS procedure above
    (demo runs from the DOS compatibility box in full screen)

  -  A 3MB logical disk needs to be set up;
     add the following line to config.sys,
     device=c:\OS2\vdisk 3072

------------------------------------------------------------------
Notes: 1. When running with XGA-2 ensure the DMQS files have been
          properly installed. These are on the XGA-2
          driver diskette and available from the DISPLAY tools disk.

       2. To exit from demo, do the following:
              hit:    ctrl, then break key
              type:   y
              hit:    Enter
              type    mode co80

              (should return to the c prompt screen)


